D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-600 | Hardware Version: A1 | Firmware Version : 1.01NA |

| Setup | Advanced | Tools | Status | Support

- Virtual Server
- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Access Control
- Website Filter
- Inbound Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- IPv6

# Firewall Settings

The Firewall Settings allows you to set a single computer on your network outside of the router.

## Firewall Settings

Enable SPI : |

## NAT Endpoint Filtering

| Endpoint Independent
UDP Endpoint Filtering : | Address Restricted
| Port And Address Restricted
| Endpoint Independent
TCP Endpoint Filtering : | Address Restricted
| Port And Address Restricted

## Anti-Spoof checking

Enable anti-spoof checking : |

## DMZ Host

The DMZ (Demilitarized Zone) option lets you set a single computer on your network outside of the router. If you have a computer that cannot run Internet applications successfully from behind the router, then you can place the computer into the DMZ for unrestricted Internet access.

Note: Putting a computer in the DMZ may expose that computer to a variety of security risks. Use of this option is only recommended as a last resort.

Enable DMZ : |
DMZ IP Address : |  |  |

## Application Level Gateway (ALG) Configuration

PPTP : |
IPSec (VPN) : |
RTSP : |
SIP : |

Helpful Hints…

Enable the DMZ option only as a last resort. If you are having trouble using an application from a computer behind the router, first try opening ports associated with the application in the Virtual Server or Port Forwarding sections.

More…

Copyright © 2004-2009 DLink, Inc.