D-LINK SYSTEMS, INC. | WIRELESS AP : SETUP / LAN SETUP

Product Page: DAP-1360 | Firmware Version: V1.01

| SETUP | ADVANCED | MAINTENANCE | STATUS | HELP

- WIZARD
- WIRELESS SETUP
- LAN SETUP
- LOGOUT

# Network Settings :

Use this section to configure the internal network settings of your AP and also to configure the built-in DHCP Server to assign IP addresses to the computers on your network. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

## LAN CONNECTION TYPE :

Choose the mode to be used by the Access Point.

My LAN Connection is : |

## STATIC IP ADDRESS LAN CONNECTION TYPE :

Enter the static address information.

IP Address : |
Subnet Mask : |
Gateway Address : |

## DYNAMIC IP (DHCP) LAN CONNECTION TYPE :

IP Address Information.

IP Address : |
Subnet Mask : |
Gateway Address : |

## DEVICE NAME (NETBIOS NAME) :

Device Name : |

## DHCP Server Settings :

Use this section to configure the built-in DHCP Server to assign IP addresses to the computers on your network.

Enable DHCP Server : |
DHCP IP Address Range : | to (addresses within the LAN subnet)
DHCP Lease Time : |

## Dynamic DHCP Client List :

Host Name | IP Address | MAC Address | Expired Time |
NONE | ---- | ---- | ---- |

Helpful Hints..
LAN Settings:
LAN Connection type:
The factory default setting is "Static IP" which allows the IP address of the DAP-1360 to be manually configured in accordance to the applied local area network. Enable Dynamic (DHCP) to allow the DHCP host to automatically assign the Access Point an IP address that conforms to the applied local area network.
IP Address:
The default IP address is 192.168.0.50. It can be modified to conform to an existing local area network. Please note that the IP address of each device in the wireless local area network must be within the same IP address range and subnet mask. Take default DAP-1360 IP address as an example, each station associated to the AP must be configured with a unique IP address falling in the range of 192.168.0.*. "*" ranges from 1 to 254 but 50 in this case.
Subnet Mask:
A mask used to determine what subnet an IP address belongs to. The default subnet setting is 255.255.255.0.
Gateway:
Specify the gateway IP address of the local network.
DHCP Server:
If you already have a DHCP server on your network or are using static IP addresses on all the devices on your network, uncheck Enable DHCP Server to disable this feature.
Device Name(NetBIOS Name):
Device Name(NetBIOS Name) allows you to configure this device more easily when your network using TCP/IP protocol. You can enter the device name of the AP into your web browser to access the instead of IP address for configuration. Recommend to change the device name if there're more than one D-Link devices within the subnet.

Copyright © 2004-2009 D-Link Systems, Inc.