> > Wizard
> > This Quick Setup will guide you through the steps necessary to configure your DSL Router.
> > ATM PVC Configuration.
> > Select the check box below to enable DSL Auto-connect process.

> > | DSL Auto-connect

> > The Virtual Path Identifier (VPI) and Virtual Channel Identifier (VCI) are needed for setting up the ATM PVC. Do not change VPI and VCI numbers unless your ISP instructs you otherwise.

> > VPI: [0-255] |
> > VCI: [32-65535] |

> > Enable Quality Of Service
> > Enabling QoS for a PVC improves performance for selected classes of applications. However, since QoS also consumes system resources, the number of PVCs will be reduced consequently. Use Advanced Setup/Quality of Service to assign priorities for the applications.

> > Enable Quality Of Service |