D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / WAN

Firmware Version: 1.32NA
Hardware Version: A4
Product Page: DIR-655

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## USB Settings

Use this section to configure your USB port. There are several configurations to choose from: Shareport and WCN Configuration.

Note : If using the Shareport option, users will need to install the Shareport Utility into their computers to share the USB device through the router.

Note: Only Administrator has access to some of these functionalities.

### USB Settings

Choose the type of USB device to be plugged into the USB port.

My plug of USB type is :

### Dynamic IP (DHCP) Internet Connection Type :

Use this Internet connection type if your Internet Service Provider (ISP) didn't provide you with IP Address information and/or a username and password.

### WWAN Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### WWAN Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPPoE Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPTP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### L2TP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

IP Address :

Subnet Mask :

Default Gateway :

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Host Name :

Use Unicasting : (compatibility for some DHCP Servers)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Country :

ISP :

Username : (optional)

Password : (optional)

Verify Password : (optional)

Dial Number :

APN :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

MTU : (bytes) (128~1492)

Address Mode : Dynamic IP Static IP

IP Address :

Username :

Password :

Verify Password :

Service Name : (optional)

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Address Mode : Dynamic IP Static IP

PPTP IP Address :

PPTP Subnet Mask :

PPTP Gateway IP Address :

PPTP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Address Mode : Dynamic IP Static IP

L2TP IP Address :

L2TP Subnet Mask :

L2TP Gateway IP Address :

L2TP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Primary DNS Server : (optional)

Secondary DNS Server : (optional)

MTU : (bytes) MTU default =

MAC Address :

### WAN Ping

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respond :

WAN Ping Inbound Filter :

Details :

### Multicast Streams

Enable Multicast Streams :

### WAN Physical setting :

Address Mode : Dynamic IP Static IP

IP Address :

Subnet Mask :

Default Gateway :

Primary DNS Server : (optional)

Secondary DNS Server : (optional)

Helpful Hints...

Device drivers and the D-Link USB Network Utility must be installed on each computer that will use the device.

If you have trouble accessing the Internet through the router. Double check the settings you entered on this page and verify with your Internet Service Provider (ISP) if needed.

For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Streams option is enabled.

More...

Copyright © 2004-2008 D-Link Systems, Inc.