D-Link Corporation. | WIRELESS INTERNET CAMERA | STATUS | DEVICE INFO

Product: DCS-920 |  | Firmware Version: 1.00

| Live Video | Setup | Maintenance | Status | Help

Device Info
Logout

# Device Info

All of your network connection details are displayed on this page. The firmware version is also displayed here.

## Basic information

Camera Name | DCS-920
Time & Date |
Firmware Version | 1.00 (2008-04-25)
IP Address | 192.168.0.20
Subnet Mask | 255.255.255.0
Default Gateway | 0.0.0.0
Primary DNS | 0.0.0.0
Secondary DNS | 0.0.0.0
DDNS | Disable
FTP Server Test | No test conducted
E-mail Test | No test conducted

## Wireless Status

Connection Mode | Infrastructure
Link | No
SSID | dlink (MAC : 00 00 00 00 00 00)
Channel | 6
Transmission Rate | 54M bps
Encryption | No

Helpful Hints.. All of your network connection details are displayed on this page.

Copyright (C) 2007-2008 D-Link Corporation.