dlink-a389e6

Product Page: DNS-343 |  | Firmware Version: 1.03

| Setup | Advanced | Maintenance | Status | Support

- RAID
- Users / Groups
- Quotas
- Network Access
- FTP Server
- UPnP AV Server
- iTunes Server
- DHCP Server
- LLTD
- Remote Backup
- Add-ons
- Logout

# REMOTE BACKUP SETTINGS :

This section allows you to backup files on the DNS-343 to one or more remote NAS devices in order to prevent data loss in the event of a failure. You can securely backup or recover your data over an encrypted SSH connection.

## REMOTE BACKUP SETTINGS :

Type | Source Destination

Password |

Source IP |
Password |
Save To |  |
Method | Keep existing file |

## SOURCE SHARE PATH :

Dest. Backup Folder Name |
Backup from |  |

## SOURCE STATUS :

Status | Stopped

## SOURCE SHARE LIST :

: Modify Settings : Delete
Backup from | Dest. Folder Name |  |  |

## DESTINATION LIST :

| Backup from | Dest. Folder Name |

Failed.

Helpful Hints..
If the DNS-343 is connected to a router, you will need to configure the router to forward port 22, port 873, and port 62057 to the IP address of this DNS-343.

Copyright © 2008-2009 D-Link Corporation/D-Link Systems, Inc.