D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / WAN

Firmware Version: 1.01
Hardware Version: A1
Product Page: DIR-825

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## WAN

Use this section to configure your Internet Connection type. There are several connection types to choose from: Static IP, DHCP, PPPoE, PPTP, and L2TP. If you are unsure of your connection method, please contact your Internet Service Provider.

Note : If using the PPPoE option, you will need to remove or disable any PPPoE client software on your computers.

Note: Only Administrator has access to some of these functionalities.

### Internet Connection Type

Choose the mode to be used by the router to connect to the Internet.

My Internet Connection is :

### Static IP Address Internet Connection Type :

Enter the static address information provided by your Internet Service Provider (ISP).

### Dynamic IP (DHCP) Internet Connection Type :

Use this Internet connection type if your Internet Service Provider (ISP) didn't provide you with IP Address information and/or a username and password.

### WWAN Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPPoE Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPTP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### L2TP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

IP Address :

Subnet Mask :

Default Gateway :

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Host Name :

Use Unicasting : (compatibility for some DHCP Servers)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Country :

ISP :

Username : (optional)

Password : (optional)

Verify Password : (optional)

Dial Number :

Authentication Protocol :

APN : (optional)

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

MTU : (bytes) (128~1492)

Address Mode : Dynamic IP Static IP

IP Address :

Username :

Password :

Verify Password :

Service Name : (optional)

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Address Mode : Dynamic IP Static IP

PPTP IP Address :

PPTP Subnet Mask :

PPTP Gateway IP Address :

PPTP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Address Mode : Dynamic IP Static IP

L2TP IP Address :

L2TP Subnet Mask :

L2TP Gateway IP Address :

L2TP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

### RIP (Routing Information Protocol)

Allows RIP to accept updates from this connection. Note that private routing information is never sent to this connection.

Enable RIP :

RIP Operating mode : V1 V2 Broadcast V2 Multicast

Router Metric :

RIP Password :

Confirm RIP Password :

Primary DNS Server : (optional)

Secondary DNS Server : (optional)

MTU : (bytes) MTU default = 1500

MAC Address :

### WAN Ping

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respond :

WAN Ping Inbound Filter :

Details :

### Multicast Streams

Enable Multicast Streams :

### WAN Physical setting :

Address Mode : Dynamic IP Static IP

IP Address :

Subnet Mask :

Default Gateway :

Primary DNS Server : (optional)

Secondary DNS Server : (optional)

Helpful Hints...

When configuring the router to access the Internet, be sure to choose the correct Internet Connection Type from the drop down menu. If you are unsure of which option to choose, contact your Internet Service Provider (ISP).

If you are having trouble accessing the Internet through the router, double check any settings you have entered on this page and verify them with your ISP if needed.

For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

If you are having trouble receiving multicast streams from the Internet, make sure the Multicast Streams option is enabled.

More...

Copyright © 2004-2008 D-Link Systems, Inc.