DWL-2700AP

Device Information
| Firmware Version: v2.00
| MAC Address: 00:13:46:9a:eb:b7

Ethernet
Get IP From: | Manual
IP address: | 192.168.0.50
Subnet Mask: | 255.255.255.0
Gateway: | 0.0.0.0
Wireless ( 802.11g)
SSID: | default
Channel: | 6
Super Mode: | Disabled
Rate: | Auto
Security Level: | Open System / Encryption Disabled

Device Info |  |  |  |
Stats |  |  |  |
Indication |  |  |  |
Client Info |  |  |  |