D-LINK SYSTEMS, INC | WIRELESS AP : STATUS / DEVICE INFO

Product Page: DAP-1360 | Firmware Version: V1.01

| SETUP | ADVANCED | MAINTENANCE | STATUS | HELP

- DEVICE INFO
- LOGS
- STATISTICS
- WIRELESS
- LOGOUT

# Device Information :

All of your Internet and network connection details are displayed on this page. The firmware version is also displayed here.

Firmware Version: V1.02 , 9, Oct, 2009

## lan

MAC Address : | 00:26:5A:C6:C9:1B
Connection : | Static IP
IP Address : | 192.168.0.103
Subnet Mask : | 255.255.255.0
Default Gateway : | 0.0.0.0

## wan

MAC Address : | 00:40:F4:03:26:D4
Connection : | Getting IP from DHCP server...
IP Address : | 0.0.0.0
Subnet Mask : | 0.0.0.0
Default Gateway : | 0.0.0.0
Primary DNS Server : |
Secondary DNS Server : |

## Wireless lan

MAC Address : | 00:26:5B:C6:C9:1A
Network Name(SSID) : | dlink
Channel : | 11
Security Type : | NONE

Helpful Hints..
Device Information:
This page displays the current information of the DAP-1360. The page will show the firmware currently loaded, wired and wireless settings applied on the unit.
LAN:
The MAC address of the Ethernet LAN connection, Connection Type being used (DHCP or Static), Subnet Mask and Default Gateway are displayed in this section.
WAN:
The MAC address of the WAN connection, Connection Type being used (DHCP, Static, PPPoE or PPTP), Subnet Mask and Default Gateway are displayed in this section.
WIRELESS LAN:
The Wireless MAC address, Wireless Network Name (SSID), Wireless Channel and Wireless Security Type are displayed in this section.

Copyright © 2004-2009 D-Link Systems, Inc.