D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: A1 | Firmware Version: 1.10

| Setup | Advanced | Tools | Status | Support

- Virtual Server
- Port Forwarding
- Application Rules
- Network Filter
- Website Filter
- Firewall Settings
- advanced Wireless
- advanced Network

# Advanced Wireless settings :

If you are not familiar with these Advanced Wireless settings, please read the help section before attempting to modify these settings.

## Advanced Wireless Settings :

802.11 b/g/n fixed Tx rate: | Auto Fixed
11b TX Rates : |
11g TX Rates : |
11n TX Rates : |
Beacon interval : | (msec, range:20~1000, default:100)
RTS Threshold : | (range: 256~2346, default:2346)
DTIM interval : | (range: 1~5, default:1)
Preamble Type : | Short Preamble Long Preamble
Protection : | Enable Disable

Helpful Hints. It is recommended that you leave these options at their default values. Adjusting them could negatively impact the performance of your wireless network.

Copyright © 2004-2005 D-Link Systems, Inc.