D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# Routing

The Routing option allows you to define static routes to specific destinations.

## 32 - STATIC ROUTING

Remaining number of rules that can be created: 32

| Interface | Destination | Subnet Mask | Gateway

Helpful Hints..

• Enable:
Specifies whether the entry will be enabled or disabled.

• Interface:
Specifies the interface -- WAN or WAN Physical -- that the IP packet must use to transit out of the router, when this route is used.

• Destination IP:
The IP address of packets that will take this route.

• Subnet Mask:
One bit in the mask specifies which bits of the IP address must match.

• Gateway:
Specifies the next hop to be taken if this route is used. A gateway of 0.0.0.0 implies there is no next hop, and the IP address matched is directly connected to the router on the interface specified: WAN or WAN Physical.

More...

Copyright © 2004-2007 D-Link Systems, Inc.