dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

# CAMERA SETUP

To manually add the camera, enter the IP address of the camera.

## CAMERA SETUP

Camera Index |
Camera Name |
Address |  | Port |
Administrator Name |  | Password |
Camera Channel |  | Protocol | TCP UDP HTTP
Vendor |  | Model |

## CAMERA SETUP

Camera Index |
Camera Name |
Address |  | Port |
Administrator Name |  | Password |
Camera Channel |  | Protocol | TCP UDP HTTP
Vendor |  | Model |

## CAMERA SETUP

Camera Index |
Camera Name |
Address |  | Port |
Administrator Name |  | Password |
Camera Channel |  | Protocol | TCP UDP HTTP
Vendor |  | Model |

## CAMERA SETUP

Camera Index |
Camera Name |
Address |  | Port |
Administrator Name |  | Password |
Camera Channel |  | Protocol | TCP UDP HTTP
Vendor |  | Model |

## CAMERA LIST

Index | Camera Name | Address | Port | Vendor | Model
1 | DCS-3410 | 192.168.0.200 | 80 | D-Link | DCS-3410
2 | DCS-6410 | 192.168.0.202 | 80 | D-Link | DCS-6410
3 |  |  | 80 | - none - | - none -
4 |  |  | 80 | - none - | - none -

Helpful Hints..
The following list briefly describes the Camera Setup menu items:
Camera Channel: Select the number of analog cameras supported by one video server from the list.
Vendor: Displays the manufacturer's name.
Auto Detection: Click to automatically detect all the information (such as camera channel, protocol used, vendor, model number) of the camera.
Note:
Some cameras will limit the login authority to the administrator only.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.