DWL-3200AP

Tool
Administrator Settings
Limit Administrator IP

You can limit the administrator login from specific IP address.
Limit Administrator IP 1
Enter an IP address that will be allowed for the administrator to login.
Limit Administrator IP 2
Enter the 2nd IP address that will be allowed for the administrator to login.

Login Settings

User Name
You can customize user name as an administrator of . The default username is "admin" with no password configured.
Old Password
Enter the old password.
New Password
Enter a password in this filed. The password is case-sensitive. "A" is a different character than "a." The length should be between 0 and 12 characters.
Confirm New Password
Type the password again to confirm it.

Console Settings

Status
Enable or disable console.
Console Protocol
Choose Telnet or SSH.
Timeout
Select the time out period.

SNMP Settings

Status
Enable or disable SNMP.
Public Community String
Enter the public community string for SNMP.
Private Community String
Enter the private community string for SNMP.
Trap Status
Enable or disable Trap.
Trap Server IP
The IP address of the SNMP manager to receive traps sent from the wireless access point.
Trap Type
You can specify what kind of trap type (System, Wireless) should be sent to the trap server.

Ping Control Setting

Status
Ping works by sending ICMP "echo request" packets to the target host and listening for ICMP echo response replies. By disabling the Ping control setting, this AP will not response to the ICMP echo request packets. Default is set to Enable.

Firmware and SSL
Firmware and SSL Certification Upload

You can upload files to the access point.
Upload Firmware From Local Hard Drive
The current firmware version is displayed above the file location field. After the latest firmware is downloaded, click on the "Browse" button to locate the new firmware. Once the file is selected, click on the "Open" and "OK" button to begin updating the firmware. While upgrading, please don't turn the power off.
Upload SSL Certification From Local Hard Drive
After you have downloaded a SSL certification to your local drive, click Browse. Select the certification and click open and upload to complete the upgrade.

Configuration File
Configuration File Upload and Download

You can upload and download configuration files of the access point.
Upload Configuration File
Browse to the saved configuration file you have in local drive and click open and upload to update the configuration.
Download Configuration File
Click download to save the current configuration file to your local disk. Note that if you save one configuration with administrator's password now, after reset your , and then update to this saved configuration file, the password will be gone

SNTP
SNTP Information / SNTP Settings
SNTP/NTP Information It displays current SNTP/NTP settings. SNTP/NTP Setting Enter the SNTP/NTP server IP, choose the time zone and enable or disable daylight saving time.