D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / Network Settings

Firmware Version: 1.12
Hardware Version: A2
Product Page: DIR-855

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## Network Settings

Use this section to configure the internal network settings of your router and also to configure the built-in DHCP Server to assign IP addresses to the computers on your network. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

Note: Only Administrator has access to these functionalities.

### WAN Port Mode

WAN Port Mode : Router Mode Bridge Mode

### Router Settings

Use this section to configure the internal network settings of your router. The IP Address that is configured here is the IP Address that you use to access the Web-based management interface. If you change the IP Address here, you may need to adjust your PC's network settings to access the network again.

Router IP Address:

Subnet Mask:

Device Name:

Default Gateway:

Primary DNS Server :

Secondary DNS Server :

Local Domain Name: (optional)

Enable DNS Relay:

### DHCP Server Settings

Use this section to configure the built-in DHCP Server to assign IP addresses to the computers on your network.

Enable DHCP Server:

DHCP IP Address Range: to

DHCP Lease Time: (minutes)

Always broadcast: (compatibility for some DHCP Clients)

NetBIOS announcement:

Learn NetBIOS from WAN:

NetBIOS Scope: (optional)

NetBIOS node type : Broadcast only (use when no WINS servers configured)

Point-to-Point (no broadcast)

Mixed-mode (Broadcast then Point-to-Point)

Hybrid (Point-to-Point then Broadcast)

Primary WINS IP Address:

Secondary WINS IP Address:

### Add DHCP Reservation

Enable:

Computer Name: <<

IP Address:

MAC Address:

### DHCP Reservations List

Enable | Computer Name | MAC Address | IP Address |  |
--- | --- | --- | --- | --- | ---

### Number of Dynamic DHCP Clients:3

Hardware Address | Assigned IP | Hostname | Expires |  |
--- | --- | --- | --- | --- | ---
e9:eb:b3:a6:db:3c | 192.168.0.194 |  | 17 Hours 55 Minutes | Revoke | Reserve
e1:6c:d6:ae:52:90 | 192.168.0.195 |  | 17 Hours 55 Minutes | Revoke | Reserve
00:04:23:2c:44:9f | 192.168.0.199 | End_User | 17 Hours 29 Minutes | Revoke | Reserve

Helpful Hints...

If you already have a DHCP server on your network or are using static IP addresses on all the devices on your network, uncheck Enable DHCP Server to disable this feature.

If you have devices on your network that should always have fixed IP addresses, add a DHCP Reservation for each such device.

More...

Copyright © 2004-2008 D-Link Systems, Inc.