D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Admin Setup
- Time and Date
- System
- Firmware
- Dynamic DNS
- System Check
- Schedules
- Log settings

# Dynamic DNS :

Dynamic DNS (Domain Name Service) is a method of keeping a domain name linked to a dynamic IP address. With most Cable and DSL connections, you are assigned a dynamic IP address and that address is used only for the duration of that specific connection.

With the DIR-330, you can setup your DDNS service and the DIR-330 will automatically update your DDNS server every time it receives a new WAN IP address.

## ddns Settings :

Enable Dynamic DNS : |
Server Address : |
Host Name : |
Username or Key : |
Password or Key : |
Verify Password or Key : |
Timeout : | (hours)
Status : | Disconnected

Helpful Hints.. In order to use this feature you must first have a DDNS account from one of the providers in the drop down menu.

Copyright © 2004-2005 D-Link Systems, Inc.