D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# QoS (Quality of Service) Engine

Use this section to configure D-Link's Smart QoS. Smart QoS improves VoIP voice quality or streaming by ensuring that your VoIP or streaming traffic is prioritized over other network traffic, such as FTP or Web. For optimum performance, please tick the "lag eliminated" option to automatically set the priority for your applications.

## Bandwidth

Uplink Speed : |
Downlink Speed : |

Please contact your Internet Service Provider to check your xDSL or cable uplink bandwidth. An accurate uplink bandwidth setting allows the QoS engine to operate smoothly and efficiently.

## QOS

Lag eliminated (VoIP, Streaming)

Helpful Hints.

• The Smart QoS feature helps improve your network VoIP and streaming performance by prioritizing the data flows of network applications.

More...

Copyright © 2004-2007 D-Link Systems, Inc.