> > WAN Setup

> > ATM PVC Configuration
> > This screen allows you to configure an ATM PVC identifier (VPI and VCI) and select a service category. Choose an existing interface by selecting the checkbox to enable it.

> > VPI: [0-255] |
> > VCI: [32-65535] |

> > Service Category: |

> > Peak Cell Rate: [cells/s] |

> > Sustainable Cell Rate: [cells/s] |
> > Maximum Burst Size: [cells] |

> > Enable Quality Of Service
> > Enabling packet level QoS for a PVC improves performance for selected classes of applications. QoS cannot be set for CBR and Realtime VBR. QoS consumes system resources; therefore the number of PVCs will be reduced. Use Advanced Setup/Quality of Service to assign priorities for the applications.

> > Enable Quality Of Service |