Wizard
Wireless
WAN
LAN
DHCP
DNS
DynamicDNS
Logout

Wireless Settings
These are the wireless settings for the AP(Access Point) Portion.
| Enable AP
SSID: |
Channel: |
Security: | None WEP WPA

Enable WEP Wireless Security
Authentication Type:
Select | Encryption Key | Cipher
Enter 10, 26, 58 hexadecimal digits(0~9,A~F) for 64, 128, or 256 bit Encryption Keys respectively. e.g., AAAAAAAAAA for a key length of 64 bits.

Please save and reboot the device to take effect !