D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: C1 | Firmware Version: 3.10NA |

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- INTERNET
- WIRELESS SETTINGS
- NETWORK SETTINGS

# WAN

Use this section to configure your Internet Connection type. There are several connection types to choose from: Static IP, DHCP, PPPoE, PPTP, L2TP. If you are unsure of your connection method, please contact your Internet Service Provider.

Note: If using the PPPoE option, you will need to remove or disable any PPPoE client software on your computers.

## Internet Connection Type

Choose the mode to be used by the router to connect to the Internet.

My Internet Connection is : |

## PPTP :

Enter the information provided by your Internet Service Provider (ISP).

Address Mode | Dynamic IP Static IP
PPTP IP Address : |
PPTP Subnet Mask : |
PPTP Gateway IP Address : |
PPTP Server IP Address : |
Username : |
Password : |
Verify Password : |
Reconnect Mode : | Always on On demand Manual
Maximum Idle Time : | (minutes, 0=infinite)
Primary DNS Address : |
Secondary DNS Address : |
MTU : | (bytes) MTU default = 1400
MAC Address : |

Helpful Hints…

When configuring the router to access the Internet, be sure to choose the correct Internet Connection Type from the drop down menu. If you are unsure of which option to choose, contact your Internet Service Provider (ISP).

If you are having trouble accessing the Internet through the router, double check any settings you have entered on this page and verify them with your ISP if needed.

More…

Copyright © 2004-2008 D-Link Systems, Inc.