D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# Wake on LAN Settings

The Wake on LAN option allows you to define the UDP port on your router that will be used to receive Magic Packets from the Internet. The Wake on LAN function allows a computer to be turned on or woken up remotely by a Magic Packet.

## Wake on LAN

Enable Wake on LAN : |
UDP Port : |

Helpful Hints..
• The Wake on LAN function can be used to remotely turn on a PC connected to the LAN side of the router. Specify the UDP port that will be used by the Wake on LAN magic packet to prevent the router from thinking the Wake on LAN request is a hostile attack and blocking it.

More...

Copyright © 2004-2007 D-Link Systems, Inc.