D-LINK SYSTEMS, INC. | WIRELESS CLIENT : Setup / Lan Setup

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

- Setup Wizard
- Wireless Setup
- Lan Setup
- Logout

## Network Settings

Use this section to configure the internal network settings of your AP.

Device Name(NetBIOS Name) allows you to configure this device more easily when your network using TCP/IP protocol. You can enter the device name of the AP into your web browser to access the instead of IP address for configuration. Recommend to change the device name if there're more than one D-Link devices within the subnet.

### Lan Connection Type

Choose the mode to be used by the Access Point.

My LAN Connection is :

### Dynamic IP(DHCP) Static IP Address Lan Connection Type

IP Address Information.

IP Address :

Subnet Mask :

Gateway Address :

### Device Name(Netbios Name)

Device Name :

Helpful Hints...

LAN Settings:
Also referred as private settings. LAN settings allow you to configure LAN interface of DAP-1350. LAN IP address is private to your internal network and is not visible to Internet. The factory default setting is Dynamic IP(DHCP).

LAN Connection type:
The factory default setting is Dynamic IP(DHCP) to allow the DHCP host to automatically assign the Access Point an IP address that conforms to the applied local area network. Enable "Static IP" which allows the IP address of the DAP-1350 to be manually configured in accordance to the applied local area network.

IP Address:
The default IP address is 192.168.0.50. It can be modified to conform to an existing local area network. Please note that the IP address of each device in the wireless local area network must be within the same IP address range and subnet mask. Take default DAP-1350 IP address as an example, each station associated to the AP must be configured with a unique IP address falling in the range of 192.168.0.*. "*" ranges from 1 to 254 but 50 in this case.

Subnet Mask:
A mask used to determine what subnet an IP address belongs to. The default subnet setting is 255.255.255.0.

Gateway:
Specify the gateway IP address of the local network.

Device Name(NetBIOS Name):
Device Name(NetBIOS Name) allows you to configure this device more easily when your network using TCP/IP protocol. You can enter the device name of the AP into your web browser to access the instead of IP address for configuration. Recommend to change the device name if there're more than one D-Link devices within the subnet.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.