> > Wireless -- Security

> > This page allows you to configure security features of the wireless LAN interface. You can sets the network authentication method, selecting data encryption, specify whether a network key is required to authenticate to this wireless network and specify the encryption strength.
> > Click "Apply" to configure the wireless security options.

> > Select SSID: |
> > Network Authentication: |

> > WPA2 Preauthentication: |

> > Network Re-auth Interval: |

> > WPA Pre-Shared Key: |  |  | Click here to display

> > WPA Group Rekey Interval: |

> > RADIUS Server IP Address: |
> > RADIUS Port: |
> > RADIUS Key: |

> > WPA Encryption: |

> > WEP Encryption: |

> > Encryption Strength: |
> > Current Network Key: |
> > Network Key 1: |
> > Network Key 2: |
> > Network Key 3: |
> > Network Key 4: |
> > | Enter 13 ASCII characters or 26 hexadecimal digits for 128-bit encryption keys
> > | Enter 5 ASCII characters or 10 hexadecimal digits for 64-bit encryption keys