D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page : DIR-685

Hardware Version : A1

Firmware Version : 1.00NA

| Setup | Advanced | Storage | Tools | Status | Support

- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Website Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- Guest Zone
- Wake on LAN

# Advanced Network Settings

If you are not familiar with these Advanced Network Settings, please read the help section before attempting to modify these settings.

## UPNP

Universal Plug and Play (UPnP) supports peer-to-peer Plug and Play functionality for network devices.

Enable UPnP : |

## WAN PING

If you enable this feature, the WAN port of your router will respond to ping requests from the Internet that are sent to the WAN IP Address.

Enable WAN Ping Respose : |

## WAN PORT SPEED

## MULTICAST STREAMS

Enable Multicast Streams : |
Wireless enhance mode : |

Helpful Hints..
• For added security, it is recommended that you disable the WAN Ping Respond option. Ping is often used by malicious Internet users to locate active networks or PCs.

More...

Copyright © 2004-2007 D-Link Systems, Inc.