D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: C1 | Firmware Version: 3.10NA |

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- INTERNET
- WIRELESS SETTINGS
- NETWORK SETTINGS

# WAN

Use this section to configure your Internet Connection type. There are several connection types to choose from: Static IP, DHCP, PPPoE, PPTP, L2TP. If you are unsure of your connection method, please contact your Internet Service Provider.

Note: If using the PPPoE option, you will need to remove or disable any PPPoE client software on your computers.

## Internet Connection Type

Choose the mode to be used by the router to connect to the Internet.

My Internet Connection is : |

## Dynamic IP (DHCP) Internet Connection Type :

Use this Internet connection type if your Internet Service Provider (ISP) didn't provide you with IP Address information and/or a username and password.

Host Name : |
DHCP routing option : |
Use Unicasting : | (compatibility for some DHCP Servers)
Primary DNS Address : |
Secondary DNS Address : |
MTU : | (bytes)MTU default = 1500
MAC Address : |

Helpful Hints…

When configuring the router to access the Internet, be sure to choose the correct Internet Connection Type from the drop down menu. If you are unsure of which option to choose, contact your Internet Service Provider (ISP).

If you are having trouble accessing the Internet through the router, double check any settings you have entered on this page and verify them with your ISP if needed.

More…

Copyright © 2004-2008 D-Link Systems, Inc.