D-LINK SYSTEMS, INC | WIRELESS AP : TOOLS / WATCHDOG

Product Page: DAP-1360 | Firmware Version: V1.01

| SETUP | ADVANCED | MAINTENANCE | STATUS | HELP

- ADMIN
- SYSTEM
- FIRMWARE
- WATCHDOG
- TIME
- SCHEDULES
- LOGOUT

# WatchDog (Ping of Life) :

The Watchdog feature pings a specified IP address. If the IP address stops responding to pings, your access point will be rebooted. You can also select an option to have the DAP-1360 send an e-mail alert if the specified IP address stops responding to pings.

## WatchDog :

Enable Watchdog (Ping of Life) : |
Update Time Interval : | (minutes, range:1-60, default:1)
Watchdog Response IP : |
Enable Mail Alert : |
SMTP Server : |
Sender E-mail : |
Receiver E-mail : |
Enable Authentication : |
Account Name : |
Password : |
Verify Password : |

Helpful Hints..
Enable Watchdog (Ping of Life):
Enable the Watchdog (Ping of Life) to check some host IP.
Update Time Interval:
The interval to ping.
Watchdog Response IP:
Pair this DAP-1360 with a device that can respond back to the pings.
Enable Mail Alert:
If you want to enable Mail Alert, you must enable Syslog first. When DAP-1360 can't ping the host IP, the DAP-1360 will send mail to the user.
SMTP server:
Please enter the mail server IP.
Mail Address:
Please enter the mail address of the user to be notified.

Copyright © 2004-2009 D-Link Systems, Inc.