dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Menu
- Live Video
- Playback
- Setup
- Maintenance
- Status
- Logout

#
HELP MENU

- User Management
- RAID
- Backup and Restore
- Firmware Update

##

Create New Users
Step 1: Input the user name of this new user.
Step 2: Input the password of this new user. And confirm the password again.
Step 3: Select the live view cameras and PTZ / IO Control function which this user can access.
Step 4: Select the playback channels and Backup Data function which this user can access.
Step 5: Click the Save Settings button to create a new user.

Note
Administrator will be the only user who can apply all the functions, and this account is not delectable. Default password of administrator password is empty, it is strongly recommend to change it when first login. If user forgets the administrator password, please press the reset button from the rear panel of the device to reset to factory default.

User list
Change User's Password
Step 1: Click the Change Password icon of the user name who you want to modify.
Step 2: Input the password of this new user. And confirm the password again.
Step 3: Click the Apply button to save. Click Cancel to abort.
Delete User
Except administrator, you can delete any users with the following steps.
Step 1: Click the Delete User icon of the user you want to delete.
Step 2: In the confirmation box, click the OK button.
Modify the Information of Users
Step 1: Click the Modify User Privileges icon from one of the users in the User List.
Step 2: Select the live view cameras and PTZ / IO Control function which this user can access.
Step 3: Select the playback channels and Backup Data function which this user can access.
Step 4: Click the Apply button to save. Click Cancel to abort.

## RAID

Choose from four different hard drive configurations in this section. Begin by pressing the Set RAID Type and Re-Format button. Note that all data will be lost during this process.StandardCreates two separate volumes (or one volume if only one hard drive is present). Each hard drive has its own volume.
JBOD (Linear)
Combines both hard drives in a linear fashion which will create one large volume geared towards maximum available space.
RAID 0
Combines both hard drives in a striped fashion which will create one large volume geared towards maximum performance.
RAID 1
Mirrors the hard drives for redundancy. If one hard drive fails, the other still has all of the data. Replace the failed hard drive and it will re-mirror, restoring maximum data protection.

##

User can save the configurations to a file or restore it once necessary. Restart the NVR can keep system work freshly. Reset the NVR will restore all configurations to factory default.
Save Configuration
All the configurations can be saved as a file to the specified location. Click Save Configuration button to save the file.
Load Configuration File
User can restore the configuration file after reset to factory default or restore from another NVR’s configuration file
Click Browse's button to select the configuration file and restore it by click Restore Configuration From File button.
Restart
If you found NVR not work properly or crash from some unknown reason, please restart NVR. Restart NVR will take about 1 and half minutes.
Reset to Default
This will reset all configurations to factory default. User can check the preserve functions from IP or DDNS, thus the remote connection will remain after reset.
Device Settings
Enter your device Name here. This name is what the DNS-726-4 will appear as on the network

##

You can upgrade the firmware of the device from this page. The firmware you want to use must be saved on the local hard drive of the computer you are working from. Click Browse button to search the local hard drive for the firmware to be used for the update. Click Apply to begin the upgrade. Please check the D-Link support site for firmware updates at D-Link Support Page.