D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-600 | Hardware Version: A1 | Firmware Version : 1.01NA |

| Setup | Advanced | Tools | Status | Support

- Virtual Server
- Port Forwarding
- Application Rules
- QoS Engine
- Network Filter
- Access Control
- Website Filter
- Inbound Filter
- Firewall Settings
- Routing
- Advanced Wireless
- Advanced Network
- IPv6

# MAC Address Filter

The MAC (Media Access Controller) Address filter option is used to control network access based on the MAC Address of the network adapter. A MAC address is a unique ID assigned by the manufacturer of the network adapter. This feature can be configured to ALLOW or DENY network/Internet access.

## 24 –– MAC Filtering Rules

Configure MAC Filtering below:

MAC Address |  | DHCP Client List |

Helpful Hints…

Create a list of MAC addresses that you would either like to allow or deny access to your network.

Computers that have obtained an IP address from the router's DHCP server will be in the DHCP Client List. Select a device from the drop down menu, then click the arrow to add that device's MAC address to the list.

Click the Clear button to remove the MAC address from the MAC Filtering list.

More…

Copyright © 2004-2009 DLink, Inc.