D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-330 | Firmware Version: 1.12

| Setup | Advanced | Maintenance | Status | Help

- Menu
- Setup
- Advanced
- Maintenance
- Status

# sTATUS Help

- Device Info
- Log
- Statistics
- Wireless Clients
- LAN Clients
- Routing
- VPN

## Device Info

All of your Internet and network connection details are displayed on the Device Info page. The firmware version is also displayed here.

Note: Some browsers have limitations that make it impossible to update the WAN status display when the status changes. Some browsers require that you refresh the display to obtain updated status. Some browsers report an error condition when trying to obtain WAN status.

Depending on the type of WAN connection, you can take one of the following sets of actions:
LAN
Displays the LAN (Local Area Network) settings of your DIR-330.

WAN
DHCP Connection – Clicking the DHCP Release button unassigns the router's IP address. The router will not respond to IP messages from the WAN side until you click the DHCP Renew button or power-up the router again. Clicking the DHCP Renew button causes the router to request a new IP address from the ISP's server.
PPPoE, PPTP, L2TP Connection– Depending on whether or not the WAN connection is currently established, you can click either the Connect button to attempt to establish the WAN connection or the Disconnect button to break the WAN connection.
BigPond Connection – Depending on whether you are currently logged into BigPond, you can click either the BigPond Login button to attempt to establish the WAN connection or the BigPond Logout button to break the WAN connection.
Russian PPPoE and PPTP – Depending on whether or not the WAN connection is currently established, you can click wither the Connect button to attempt to establish the WAN connection or the Disconnect button to break the WAN connection. In the WAN Physical section, clicking the DHCP Release button unassigns the router’s IP address. The router will not respond to IP messages from the WAN side until you click the DHCP Renew button or power-up the router again. Clicking the DHCP Renew button causes the router the request a new IP address from the ISP’s server.
Wireless
This displays the SSID, Channel, and whether or not Encryption is enabled on the Wireless interface.

## Log

Log Files
The DIR-330 keeps a running log of events and activities occurring on it at all times. The log will display up to 200 recent logs. Newer log activities will overwrite the older logs. You can save the log files or have them emailed to you by clicking on the Log Settings menu that is located within the Maintenance section. This is recommended as the logs are cleared every time the router is rebooted.
First Page - Click this button to go to the first page of the log.
Last Page - Click this button to go to the last page of the log.
Previous - Moves back one log page.
Next - Moves forward one log page.
Clear - Clears the logs completely.

## Statistics

Displays LAN, WAN, and Wireless packet statistics. Transmitted –The number of packets sent from the router. Received –The number of packets received by the router.

## Active Session

The Active Session Status menu shows the active sessions currently running on your router. The list will display the protocol, the source IP address and the destination IP address for each active session. Click the buttons at the top of the list to toggle between pages of the list or to refresh the list.

## Wireless Clients

Displays current wireless clients connected to your DIR-330.

## LAN Clients

Displays current wired clients connected to your DIR-330

## Routing

The Routing Status menu shows information about the routes that have been enabled on your router. The list will display the destination IP address, gateway IP address, subnet mask, metric and interface for each route.

## VPN

Displays current established VPN tunnels.

Copyright © 2004-2005 D-Link Systems, Inc.