D-LINK SYSTEMS, INC. | WIRELESS AP : SETUP / WIRELESS SETUP

Product Page: DAP-1360 | Firmware Version: V1.01

| SETUP | ADVANCED | MAINTENANCE | STATUS | HELP

- WIZARD
- WIRELESS SETUP
- LAN SETUP
- LOGOUT

# WIRELESS NETWORK

Use this section to configure the wireless settings for your D-Link Access Point. Please note that changes made on this section may also need to be duplicated on your wireless client.

To protect your privacy you can configure wireless security features. This device supports three wireless security modes including: WEP or WPA and WPA2.

## Wireless Network Settings :

Enable Wireless : |
Wireless Mode : |
Wireless Type : |
Wireless Network Name : | (Also called the SSID)
Enable Auto Channel Scan : |
Wireless Channel : |
802.11 Mode : |
Channel Width : |
Transmission Rate : |
Enable Hidden Wireless : | (Also called Disable SSID Broadcast)

## Wireless MAC Clone :

Enable : |
MAC Source : |
MAC Address : |

| MAC Address

## Wireless Security Mode :

Security Mode : |

## WEP :

WEP is the wireless encryption standard. To use it you must enter the same key(s) into the AP and the wireless stations. For 64 bit keys you must enter 10 hex digits into each key box. For 128 bit keys you must enter 26 hex digits into each key box. A hex digit is either a number from 0 to 9 or a letter from A to F. For the most secure use of WEP set the authentication type to "Open Key" when WEP is enabled.

You may also enter any text string into a WEP key box, in which case it will be converted into a hexadecimal key using the ASCII values of the characters. 5 text characters can be entered for 64 bit keys, and 13 characters for 128 bit keys.

Authentication : |
WEP Encryption : |
Key Type : |
Default WEP Key : |
WEP Key 1 : |
WEP Key 2 : |
WEP Key 3 : |
WEP Key 4 : |

## WPA :

WPA requires stations to use high grade encryption and authentication.

## WPA2 :

WPA2 requires stations to use high grade encryption and authentication.

## WPA2-auto :

WPA2-Auto requires stations to use high grade encryption and authentication.

Cipher Type : |
PSK / EAP : |

Passphrase : |
Confirmed Passphrase : |

RADIUS Server 1 : | IP |
| Port |
| Shared Secret |
RADIUS Server 2 : | IP |
| Port |
| Shared Secret |

## BRIDGE setting :

Bridge Security: |
WEP Key: |
Passphrase: (8~63 char.) |

## WAN Settings :

This page is used to configure the parameters for Internet network which connects to the WAN port of your Access Point. Here you may change the access method to static IP, DHCP, PPPoE or PPTP by click the item value of WAN Access type.

My Internet Connection is: |

IP Address: |
Subnet Mask: |
Default Gateway: |
MTU Size: | (bytes) MTU default = 1500

Host Name: |
MTU Size: | (bytes) MTU default = 1500

Username: |
Password: |
Verify Password: |
Service Name: | (optional)
Reconnection Type: |
Maximum Idle Time: | (1-1000 minutes)
MTU Size: | (bytes) MTU default = 1500

PPTP IP Address: |
PPTP Subnet Mask: |
PPTP Server IP Address: |
Username: |
Password: |
Verify Password: |
MTU Size: | (bytes) MTU default = 1400

| Attain DNS Automatically
| Set DNS Manually

Primary DNS Server: |
Secondary DNS Server: |

Clone MAC Address: |

## WIFI PROTECTED SETUP (ALSO CALLED WCN 2.0 IN WINDOWS VISTA) :

Enable : |

Lock Wireless Security : |
Current PIN : |
Wi-Fi Protected Status : |

Helpful Hints..
Wireless Mode:
Select a function mode to configure your wireless network. Function wireless modes include Access Point, AP Client, Bridge, Bridge with AP, Repeater, WISP Client Router and WISP Repeater. Function wireless modes are designed to support various wireless network topologies and applications.
Wireless Network Name:
Changing your Wireless Network Name is the first step in securing your wireless network. We recommend that you change it to a familiar name that does not contain any personal information.
Hidden Wireless:
Enabling Hidden Mode is another way to secure your network. With this option enabled, no wireless clients will be able to see your wireless network when they perform scan to see what's available. In order for your wireless devices to connect to your AP, you will need to manually enter the Wireless Network Name on each device.
Security Keys:
If you have enabled Wireless Security, make sure you write down WEP Key or Passphrase that you have configured. You will need to enter this information on any wireless device that you connect to your wireless network.
Bridge setting:
If you want to bridge with the other Bridge AP, please write down the MAC address of the Bridge AP. Besides, you also need to write down the MAC address of your Bridge AP to the other one.
Bridge Security:
If you have enabled the Bridge Security, make sure you write down WEP Key or Passphrase that you have configured. You will need to enter this information on any Bridge AP that you want to bridge with.
More...

Copyright © 2004-2009 D-Link Systems, Inc.