D-LINK SYSTEMS, INC. | WIRELESS AP : Advanced / Advanced Wireless

Firmware Version : 1.10NA
Hardware Version : A1
Product Page : DAP-1350

| Setup | Advanced | Maintenance | Status | Help

## Advanced Wireless

These options are for users that wish to change the behaviour of their 802.11n wireless radio from the standard setting. D-link does not recommend changing these settings from the factory default. Incorrect settings may impair the performance of your wireless radio. The default settings should provide the best wireless radio performance in most environments.

Note: Only Administrator has access to some of these functionalities.

### Advanced Wireless Settings

Transmit Power :

Beacon Period : (20..1024)

DTIM Interval : (1..255)

RTS Threshold : (1..2347)

Fragmentation Threshold : (256..2346)

WMM Enable :

Short GI :

IGMP Snooping :

WLAN Partition :

Helpful Hints...

Advanced Wireless:
It is recommended that you leave these options at their default values. Adjusting them could negatively impact the performance of your wireless network.
The options on this page should be changed by advanced users or if you are instructed to by one of our support personnel, as they can negatively affect the performance of your Access Point if configured improperly.

Transmit Power:
You can lower the output power of the DAP-1350 by selecting lower percentage Transmit Power values from the drop down. Your choices are: 100%, 50%, 25%, and 12.5%.

Beacon Interval:
Beacons are packets sent by an Access Point to synchronize a wireless network. Specify a Beacon interval value between 20 and 1024. The default value is set to 100 milliseconds.

DTIM Interval:
Enter a value between 1 and 255 for the Delivery Traffic Indication Message (DTIM). A DTIM is a countdown informing clients of the next window for listening to broadcast and multicast messages. When the Access Point has buffered broadcast or multicast messages for associated clients, it sends the next DTIM with a DTIM Interval value. AP clients hear the beacons and awaken to receive the broadcast and multicast messages. The default value for DTIM interval is set to 1.

Copyright © 2009 D-Link Corporation/D-Link System, Inc.