D-Link Print Server - Setup Network

Product Page: DPR-1260 | Firmware Version: 1.24

| Status | Scan | Advanced | Setup | Help

- Print Wizard
- Network Settings
- Wireless Settings
- Administration
- Firmware

# Network Setup

These are the settings of the LAN (Local Area Network) interface for the device. These settings may be referred to as "private settings". You may change the LAN IP address if needed. The LAN IP address is private to your internal network and cannot be seen on the Internet. The default IP address mode is DHCP.

## Network Settings

IP address mode | DHCP Static

IP Address |
Subnet mask |
Default gateway |

Primary DNS Server |
Secondary DNS Server |

Administrator password |
Server Name |

Helpful Hints.. Network Settings: IP address mode - Select "DHCP" to get the IP settings automatically from a DHCP server on your network. Select "Static" to use the IP settings specifed below.

IP address - Type the desired "Static" IP address of the print server. Subnet mask - The subnet mask specifies the network number portion of an IP address. Default gateway - This is the IP address of the gateway that connects the network to the internet.

Copyright © 2006 D-Link Systems, Inc.