Wizard
Wireless
WAN
LAN
DHCP
DNS
DynamicDNS
Logout

DHCP Settings
The device can be setup as a DHCP Server to distribute IP addresses to the LAN network.
| No DHCP | Choose this option. The IP address must be manually assigned at each device connected to DSL-G604T.
| DHCP Server | Choose this option to setup as a DHCP server to distribute IP addresses to the LAN network.

DHCP Server | DHCP Relay
| Starting IP Address |
| Ending IP Address |
| Lease Time | seconds
| DHCP Relay IP |
| DNS Mode | Auto Manual
| Primary DNS |
| Secondary DNS |
| Static IP Assignment
| MAC Address | IP Address
Static IP1: |  |
Static IP2: |  |
Static IP3: |  |
Static IP4: |  |
Static IP5: |  |
Enter MAC Address format as xx-xx-xx-xx-xx-xx, i.e: 00-0C-6E-D5-11-22, and IP Address format as yyy.yyy.yyy.yyy, i.e: 192.168.1.2

DHCP Clients List
Number | IP Address | MAC Address
192.168.1.2 | 00:0d:56:66:4a:61