D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Advanced / QoS Engine

Firmware Version: 2.21
Hardware Version: B2
Product Page: DIR-615

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## QoS Engine

Use this section to configure D-Link's QoS Engine. The QoS Engine improves your online gaming experience by ensuring that your game traffic is prioritized over other network traffic, such as FTP or Web. For best performance, use the Automatic Classification option to automatically set the priority for your applications.

### WAN Traffic Shaping

Enable Traffic Shaping:

Automatic Uplink Speed :

Measured Uplink Speed : Not Estimated

Manual Uplink Speed : kbps <<

Connection Type :

Detected xDSL or Other Frame Relay Network : No

### QoS Engine Setup

Enable QoS Engine :

Automatic Classification :

Dynamic Fragmentation :

### 10 -- QoS Engine Rules

| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to
| Name | Priority (1..255) | Protocol <<
Local IP Range to | Local Port Range to
Remote IP Range to | Remote Port Range to

Helpful Hints...

If the Measured Uplink Speed is known to be incorrect (that is, it produces suboptimal performance), disable Automatic Uplink Speed and enter the Manual Uplink Speed. Some experimentation and performance measurement may be required to converge on the optimal value.

More...

Copyright © 2004-2007 D-Link Systems, Inc.