D-LINK SYSTEMS, INC | WIRELESS ROUTER | HOME

Product Page: DIR-615 | Hardware Version: A1 | Firmware Version: 1.10

| Setup | Advanced | Tools | Status | Support

- Admin
- Time
- System
- Firmware
- DDNS
- SYSTEM CHECK
- SCHEDULES
- Log settings

# Fast Ethernet Virtual Cable Tester (VCT)

Cable Test is an advanced feature that integrates a LAN cable tester on every Ethernet port on the router.

## VCT INFO

Ports | Link Status |  |
WAN |  | Disconnected |
LAN1 |  | 100Mbps full Duplex |
LAN2 |  | Disconnected |
LAN3 |  | Disconnected |
LAN4 |  | Disconnected |

## Ping Test

Ping Test sends "ping" packets to test a computer on the Internet.

Host Name or IP Address: |

## Ping Result

Enter a host name or IP address above and click 'Ping'

Copyright © 2004-2005 D-Link Systems, Inc.