dlink-ECEA07

Product Page: DNS-323 |  | Firmware Version: 1.09

| SETUP | ADVANCED | TOOLS | STATUS | SUPPORT

- USERS / GROUPS
- QUOTAS
- NETWORK ACCESS
- FTP SERVER
- UPnP AV SERVER
- iTunes SERVER
- DHCP SERVER
- LLTD
- ADD-ONS
- LOGOUT

# FTP SERVER SETTINGS :

This section contains the configuration settings for the build in FTP server. The server is easy to configure and allows up to 10 users to access the server locally or remotely at the same time.

## FTP ACCOUNT SETTINGS :

Category | User Group
Group |
User | All accounts
Folder | Root
Permission |  |

## FTP SERVER SETTINGS :

Max. User |
Idle Time | (1~10 Minutes)
Port | (1025 to 3688, 3690 to 49999, 65501 to 65535, Default: 21)
Passive Mode | Use the default port range (55536-55663) Use the following port range: ~
| Report external IP in Passive mode External IP : . . .
Client Language |  |
Flow Control | Unlimited x 10 KBs |
SSL/TLS | Allow SSL/TLS connection only |

## FTP ACCESS LIST :

:R/W : Read/Write :Read Only :Modify settings :Delete
Path | User/Group | R/W |  |

## FTP Server Status :

| Status | Stopped
| Port | 21
| Max. User | 10
| Flow Control | Unlimited
| Idle Time | 2
| Client Language | Western European
| SSL/TLS connection | No
| Passive Mode |

Helpful Hints..

If your DNS-323 is connected to a router, you will need to forward port 21 (in the router configuration) to the IP address of the DNS-323.From the outside world, remember to access this FTP server by using the WAN address of your router. The default FTP port is 21. However, your can also use ports: 1025 to 3688 ,3690 to 49999, and 65501 to 65535.
In order to use FXP (File Exchange Protocol) for server-to-server data transfer, please make sure to change the port from 21 to some other port as listed in the Port section of the web UI. Also, please make sure to open the corresponding port on your router and forward that port from your router to the DNS-323.

Copyright © 2006-2009 D-Link Corporation/D-Link Systems, Inc.