Advanced Wireless Settings

Wireless Band |
Frequency |
Channel |
Data Rate |
Beacon Interval (20 - 1000) |
DTIM (1 - 255) |
Fragment Length (256 - 2346) |
RTS Length (256 - 2346) |
Transmit Power |
Super Mode |
Radio |
WMM |
Preamble |
Wireless B/G Mode |
Antenna Diversity |
IGMP Snooping |

Advance Data Rate Settings in 802.11b/g
Enable Data Rate Control | Disable | Enable
Data Rate (Mb/sec) | 1Mb/sec |  | 2Mb/sec |
| 5.5Mb/sec |  | 11Mb/sec |
| 6Mb/sec |  | 9Mb/sec |
| 12Mb/sec |  | 18Mb/sec |
| 24Mb/sec |  | 36Mb/sec |
| 48Mb/sec |  | 54Mb/sec |