D-LINK SYSTEMS, INC. | WIRELESS ROUTER : Setup / WAN

Firmware Version: 2.21
Hardware Version: B2
Product Page: DIR-615

| Setup | Advanced | Tools | Status | Support

## Reboot needed

Your changes have been saved. The router must be rebooted for the changes to take effect. You can reboot now, or you can continue to make other changes and reboot later.

## Configuration Warnings

## WAN

Use this section to configure your Internet Connection type. There are several connection types to choose from: Static IP, DHCP, PPPoE, PPTP, L2TP, and BigPond. If you are unsure of your connection method, please contact your Internet Service Provider.

Note : If using the PPPoE option, you will need to remove or disable any PPPoE client software on your computers.

### Internet Connection Type

Choose the mode to be used by the router to connect to the Internet.

My Internet Connection is :

### Static IP Address Internet Connection Type :

Enter the static address information provided by your Internet Service Provider (ISP).

### Dynamic IP (DHCP) Internet Connection Type :

Use this Internet connection type if your Internet Service Provider (ISP) didn't provide you with IP Address information and/or a username and password.

### Big Pond Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPPOE Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### PPTP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

### L2TP Internet Connection Type :

Enter the information provided by your Internet Service Provider (ISP).

IP Address :

Subnet Mask :

Default Gateway :

Host Name :

Use Unicasting : (compatibility for some DHCP Servers)

BigPond Server :

BigPond User Id :

BigPond Password :

Verify Password :

Address Mode : Dynamic IP Static IP

IP Address :

Username :

Password :

Verify Password :

Service Name : (optional)

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

Address Mode : Dynamic IP Static IP

PPTP IP Address :

PPTP Subnet Mask :

PPTP Gateway IP Address :

PPTP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

Address Mode : Dynamic IP Static IP

L2TP IP Address :

L2TP Subnet Mask :

L2TP Gateway IP Address :

L2TP Server IP Address :

Username :

Password :

Verify Password :

Reconnect Mode : Always on On demand Manual

Maximum Idle Time : (minutes, 0=infinite)

Primary DNS Server : (optional)

Secondary DNS Server : (optional)

MTU : (bytes) MTU default = 1500

MAC Address :

Helpful Hints...

When configuring the router to access the Internet, be sure to choose the correct Internet Connection Type from the drop down menu. If you are unsure of which option to choose, contact your Internet Service Provider (ISP).

If you are having trouble accessing the Internet through the router, double check any settings you have entered on this page and verify them with your ISP if needed.

More...

Copyright © 2004-2007 D-Link Systems, Inc.