D-LINK SYSTEMS, INC | WIRELESS AP | HELP

# Help MENU

Maintenance
Device Administration Enter a password in the Access Point Password field. Type the password again in the next field to confirm it. The Password is case-sensitive ("A" is a different character than "a",) and must be between 0 and 15 characters in length.

Save and Restore
The current system settings can be saved as a file onto the local hard drive. The saved file or any other saved settings file created by a DAP-1360 can be uploaded to the unit. To reload a system settings file, click on Browse to search the local hard drive for the file to be used. The device can also be reset back to factory default settings by clicking on Restore. Use the restore feature only if necessary. This will erase all previously saved settings. Make sure to save your system settings before doing a factory restore.
Save – Click this button to save the configuration file from the Access Point.
Browse – Click Browse to locate a saved configuration file and then click to Load to apply these saved settings to the Access Point.
Restore Device – Click this button to restore the Access Point to its factory default settings.

Firmware Update
You can upgrade the firmware of the device using this tool. Make sure that the firmware you want to use is saved on the local hard drive of the computer. Click on Browse to search the local hard drive for the firmware to be used for the update. Upgrading the firmware will not change any of your system settings but it is recommended that you save your system settings before doing a firmware upgrade. Please check the D-Link support site for firmware updates at http://support.dlink.com.tw/ .

WatchDog(Ping of Life)
Enable Watchdog (Ping of Life) – Enable the Watchdog (Ping of Life) to check some host IP.
Update Time Interval – The interval to ping.
Watchdog Response IP – Pair this DAP-1360 with a device that can respond back to the pings.
Enable Mail Alert – If you want to enable Mail Alert, you must enable Syslog first. When DAP-1360 can't ping the host IP, the DAP-1360 will send mail to the user.
SMTP server – Please enter the mail server IP.
Mail Address – Please enter the mail address of the mail server.

Copyright © 2004-2009 D-Link Systems, Inc.