dlink-6CE02A

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

# EVENT SETUP

Select the camera from the Camera List, and then choose one of the following three events. Connection Lost, Motion Detected or External Input.

## EVENT ACTION MANAGER

Camera List | Event & Action

- Output
- E-Mail

Action | Options
--- | ---

Helpful Hints..

Connection Lost: When a connection between the camera and NVR is lost, the NVR triggers an action.
Motion Detected: When video motion is detected, the camera triggers an action.
Input: Any external input can trigger an action. Output: When an event occurs, the system sends out an output signal to other connected devices.
E-Mail: When an event occurs, the system will send e-mail notifications. Ensure to add an e-mail address first.
Notes
- When configuring the Motion Detected event, ensure to setup the motion detection function in your camera first.
- You can also set up an event action, when the hard disk space is full.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.
Contact List
Event Configuration
Enable Event
Activation PeriodAlways Active
Activate according to set schedule
: to :
IO Type N/O
N/C
Digital Output List