D-LINK SYSTEMS, INC | WIRELESS ROUTER | TOOLS

Product Page: DIR-451 | Hardware Version: A1 | Firmware Version: v1.03_NA

| Setup | Advanced | Tools | Status | Support

- Admin
- Time
- System
- Firmware
- DDNS
- SYSTEM CHECK
- SCHEDULES
- Log settings
- Syslog
- Email Settings
- Routing

# Fast Ethernet Virtual Cable Tester (VCT) :

Cable Test is an advanced feature that integrates a LAN cable tester on every Ethernet port on the router.

## VCT INFO :

Ports | Link Status |
LAN1 |  | Disconnected, No cable detected
LAN2 |  | Disconnected, No cable detected
LAN3 |  | Disconnected, No cable detected
LAN4 |  | Connected, 100Mbps, full-duplex

## Ping Test :

Ping Test is used to send "Ping" packets to test if a computer is on the Internet.

Host Name or IP Address : |

## Ping Result:

Copyright © 2004-2008 D-Link Systems, Inc.