> > Wizard
> > WAN IP Settings

> > Enter information provided to you by your ISP to configure the WAN IP settings.
> > Notice: DHCP is not supported in IPoA mode. Changing the default gateway or the DNS effects the whole system. Configuring them with static values will disable the automatic assignment from other WAN connection.

> > WAN IP Address: |
> > WAN Subnet Mask: |

> > Obtain default gateway automatically:
> > Use the following default gateway:
> > | Use IP Address: |
> > | Use WAN Interface: |

> > Use the following DNS server addresses:
> > | Primary DNS server: |
> > | Secondary DNS server: |