dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Wizard
- Network Setup
- Camera Search
- Camera Setup
- Audio and Video
- Live & Playback Setup
- Recording Schedule
- Event Setup
- E-Mail Setup
- Dynamic DNS
- Time and Date Setup
- Logout

# AUDIO AND VIDEO

You may wish to modify the parameters in this page or directly go to the camera web site. The NVR will display all the necessary information of the selected camera.

## CAMERA PARAMETER

Camera Name | DCS-3410
Video Format | Motion JPEG MPEG4
Frame Rate |
Resolution |
Bitrate |
Audio | Enable Audio

## CAMERA PARAMETER

Camera Name | DCS-6410
Video Format | Motion JPEG MPEG4
Frame Rate |
Resolution |
Bitrate |
Audio | Enable Audio

## CAMERA PARAMETER

Camera Name |
Video Format | Motion JPEG MPEG4
Frame Rate |
Resolution |
Bitrate |
Audio | Enable Audio

## CAMERA LIST

Index | Camera Name | Address | Vendor | Model | Original Web
1 | DCS-3410 | 192.168.0.200 | D-Link | DCS-3410 | Go To Web
2 | DCS-6410 | 192.168.0.202 | D-Link | DCS-6410 | Go To Web
3 |  |  | - none - | - none - | Go To Web
4 |  |  | - none - | - none - | Go To Web

Helpful Hints..
The following list briefly describes the Camera Setup menu items:
Camera Channel: Select the number of analog cameras supported by one video server from the list.
Vendor: Displays the manufacturer's name.
Auto Detection: Click to automatically detect all the information (such as camera channel, protocol used, vendor, model number) of the camera.
Note:
Some cameras will limit the login authority to the administrator only.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.