Help

## Status

Device Information

This page displays the camera setting such as the Firmware version, MAC address, IP address, Subnet Mask, and Default Router information.

Log

Enable remote log - This option enables the camera to send camera log files to a remote server.
IP Address - The IP address of the remote server.
Port - The port number of the remote log server. The default port is 514.
Current log - View the system log file. The content of the file reveals useful information about camera configuration and connectivity status after the camera boots up.