Help of Configuration

System

System Device
| In this field, you can configure the basic information of your print server.
| Server Name : Assign a name to the print server.
| Location (optional) : Assign a location for the print server.
| Admin Contact (optional) : Assign the Admin Contact's name for the print server.

Password : | Enter the Administrator password (3-8 characters).
| To set up the password, please enter the password in the New Password box, and then enter the same one again in the Confirm Again box.

Port Setting
| In this field, you can assign the Port Name for the print server, and the description for the USB port. It also allows you to select the PJL Printer setting (Yes or No). NOTE: PJL (Print Job Language) has certain job requirements that must be met to work correctly. For more information, please refer to your printer's manual.

TIP : | Once you have changed the settings in each option, click Apply to store the settings, or Cancel to abandon.

Wireless

Wireless Interface

Connection Mode : | Select one of the two connection modes.
| Infrastructure (default) - Connects to compatibly configured wireless AP or router in a WLAN.
| Ad-Hoc - Connect to compatibly configured wireless clients in the peer-to-peer mode.

| SSID : Assign the SSID in this box. You can manually input the name or select one from the pull-down menu. To search the available wireless AP within the network, click the Site Survey button.
| Wireless Channel : Select the channel from the pull-down menu. The default setting is 6.
| Transmission Rate : Select the data transmit rate from the pull-down menu. The default setting is Fully Automatic.

WEP Encryption
| This field allows you to configure the settings of data encryption. Please remember that the WEP key must be set before the data encryption is enforced.
| WEP Encryption : This option allows you to select Disable, 64 bits, and 128 bits for the encryption setting.
| WEP Key Format : You can decide the network key to be encoded by ASCII (ASCII characters) or HEX (hexadecimal digitals). 64 bit WEP encryption uses a 10 hexidecimal character key. 128 bit WEP uses a 26 hexidecimal character key. The WEP encryption key must match the WEP settings on your AP or wireless router to connect properly. Then, enter the key(s) for the network in the Key box (1~4).

Advanced Setting
| Beacon Interval : Enter the number of beacon interval time in millisecond.

Preamble : | This option allows you to set the length of preamble.
| Setting options are: Long - it is set to 144 bits; Short - it is set to 72 bits.

| Authentication Type : You can set the authentication type by selecting the settings : Open System, Shared Key, and Both.

TIP : | Once you have changed the settings in each option, click Apply to store the settings, or Cancel to abandon.

Network

TCP/IP
| This field contains three options that allow you to configure the TCP/IP setting: IP Address, UPnP, and MAC Rendezvous.
| IP Addres : This option allows you to set the IP address manually or automatically. When you choose Manually Assign,you should enter the related information in the following boxes, including IP Address, Subnet Mask, and Default Gateway.
| UPnP : This option allows you to enable or disable UPnP mode.
| MAC Rendezvous : This option allows you to enable or disable MAC Rendezvous mode.

Microsoft Network
| Enter the name of the Workgroup that you want the print server associated with in this field.

AppleTalk
| Enter the AppleTalk Zone name in the box. In the following options, enter the related configuration, such as the printer type.
| USB
| Chooser Name : Display the print server's port name.
| Printer Type : Enter the printer's type in this box.
| PostScript Level : Select from the pull-down menu (Level 1 or Level 2).
| Font Group : Select from the pull-down menu.

TIP : | Once you have changed the settings in each option, click Apply to store the settings, or Cancel to abandon.

User

Printing Control
| By configuring the Enable User Printing Control option (Yes or No), the user in the User List is permitted to access the print server or not. For the user(s) who is not in the User List, will not be allowed to access the print server.

TIP : | Once you have changed the settings in each option, click Apply to store the settings, or Cancel to abandon.

Define Users
| You can add/delete the user(s) to/from the User List. The User List at the bottom of the screen displays the current defined user and related information for the print server.

SNMP

SNMP Management
| SNMP (Simple Network Management Protocol) is a set of protocols for managing complex networks.
| Community 1/2/3 : Enter a name in the Name box, and configure the Access Right by selecting Read Only or Read/Write from the pull-down menu.

TIP : | Once you have changed the settings in each option, click Apply to store the settings, or Cancel to abandon.