D-Link Corporation. | WIRELESS INTERNET CAMERA | SETUP | VIDEO

Product: DCS-920 |  | Firmware Version: 1.00

| Live Video | Setup | Maintenance | Status | Help

Wizard
Network Setup
Wireless Setup
Dynamic DNS
Image Setup
Video
Mail
FTP
Time and Date
Logout

# Video

In this section, you can configure the camera video quality, resolution, and frame rate.

## VIDEO PROFILE

Encode Type | Resolution | FPS | Jpeg Quality
JPEG |  |  |

## Light Frequency

50 Hz 60 Hz

Helpful Hints..
Resolution - 3 settings are available.
1.QQVGA @ 160x120 - Usually used for display on handheld devices.
2.QVGA @ 320x240 - Standard resolution for mobile phones, and PDAs
3.VGA @ 640x480 - Standard resolution for computer display.
FPS (Frames Per Second) - Highest FPS represents highest refresh rate a picture is updated on screen every second, and provides better quality of video.
Jpeg Quality - Default value is Medium.
Light Frequency - 2 options, 50 or 60 Hz. Default value is 60 Hz.

Copyright (C) 2007-2008 D-Link Corporation.