D-LINK SYSTEMS, INC | WIRELESS ROUTER | SUPPORT

# SUPPORT MENU

Status

Device Info
This page displays the current information for the DIR-451. The page will show the version of the firmware currently loaded in the device.
LAN (Local Area Network) - This displays the MAC Address of the Ethernet LAN interface, the IP Address and Subnet Mask of the LAN interface, and whether or not the router's built-in DHCP server is Enabled or Disabled.
WAN (Wide Area Network) - This displays the MAC Address of the WAN interface, as well as the IP Address, Subnet Mask, Default Gateway, and DNS server information that the DIR-451 has obtained from your ISP. It will also display the connection information that is used establish a connection with your ISP. There will be buttons for connecting and disconnecting the WWAN session.
Wireless 802.11g - This displays the SSID, Channel, and whether or not Encryption is enabled on the Wireless interface.

Log
The DIR-451 keeps a running log of events and activities occurring on it at all times. The log will display up to 200 recent logs. Newer log activities will overwrite the older logs. You can save the log files or have them emailed to you by clicking on the Log Settings button . This is recommended as the logs are cleared every time the router is rebooted.
First Page - Click this button to go to the first page of the log.
Last Page - Click this button to go to the last page of the log.
Previous - Moves back one log page.
Next - Moves forward one log page.
Clear - Clears the logs completely.

Stats
The DIR-451 keeps statistic of the data traffic that it handles. You are able to view the amount of packets that the router has Received and Transmitted on the WAN, LAN, and Wireless interfaces.
Refresh - Click this button to update the counters.
Reset - Click this button to clear the counters. The traffic counter will reset when the device is rebooted.

Wireless Use this page in order to view how many wireless clients have associated with the DIR-451. This page shows the MAC address of each associated client, how long they have been associated, and the mode they are connecting in (802.11b or802.11g).

Copyright © 2004-2008 D-Link Systems, Inc.