> > Local Area Network (LAN) Setup
> > Configure the DSL Router IP Address and Subnet Mask for LAN interface. Save button only saves the LAN configuration data. Save/Reboot button saves the LAN configuration data and reboots the router to make the new configuration effective.

> > IP Address: |
> > Subnet Mask: |

> > Enable UPnP

> > Enable IGMP Snooping
> > Standard Mode
> > Blocking Mode

> > Disable DHCP Server
> > Enable DHCP Server
> > Start IP Address: |
> > End IP Address: |
> > Leased Time (hour): |

> > Enable DHCP Server Relay
> > DHCP Server IP Address: |

> > Configure the second IP Address and Subnet Mask for LAN interface

> > IP Address: |
> > Subnet Mask: |