dlink-6CE05B

Product Page: DNS-726-4 |  | Firmware Version: 1.00

| Live Video | Playback | Setup | Maintenance | Status | Help

- Camera Status
- Device Info
- System Log
- NVR Log
- Logout

# CAMERA STATUS

This page displays the camera and recording status of the camera.

## CAMERA STATUS

Index | Name | Address | Connection Status | Recording Status | Frame Rate | Bitrate
1 | DCS-3410 | 192.168.0.200 | Connected | No Recording | 29.3 fps | 2068.6 Kbps
2 | DCS-6410 | 192.168.0.202 | Connected | No Recording | 32.2 fps | 2218.4 Kbps
3 |  |  | Disconnect | No Recording |  |
4 |  |  | Disconnect | No Recording |  |

Total Bit Rate:4287 Kbps
Last update on Thu Jun 18 2009 14:11:12
GMT-0700 (Pacific Daylight Time)

## DISK STATUS

Total Hard Drive Capacity: | 244147 MB
Unused Space: | 244070 MB
Estimated Total Recording Time: | N/A
Estimated Remaining Recording Time: | N/A

Helpful Hints..

The following list briefly describes the Camera and Recording Status menu items:
Connection Status: Click Connect or Disconnect to change the connection status.
Recording Status: Set the recording schedule of the camera.
Frame Rate: Displays the frame rate of the camera.
Bit Rate: Displays the transmission bit rate of the camera.

Copyright © 2008 D-Link Corporation/D-Link System, Inc.