InS_StArT
DE320ODI.COM
1.0
^D-Link DE-320,DE320ODI.COM,00M
?Please select the options that match your board's IO settings.
!O00M(SLOT)
1
2
3
4
5
6
7
8
$O00M(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*R00M(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
