   Windows NT 3.51 

   Introduction:
   -------------
   This document describes the procedure to install  Windows NT v3.51 
   driver for D-Link DFE-538TX 10/100 Adapter.

   Location of Driver:     \WINNT351\DLKRTS.SYS

   Installing driver procedure on Microsoft Windows NT :
   -----------------------------------------------------
   When you are in Windows NT :
   1. In the Main group of NT, select the "Control Panel" icon.

   2. In the Control Panel window, choose the "Network" icon.

   3. In the Network Settings dialog box, choose the "Add Adapter" button.
      The Add Network Adapter dialog box appears.

   4. In the list of network cards, select "<other> Requires disk from
      manufacturer", and then press <Enter> button.

   5. Insert the driver disk in CD-ROM drive, enter drive and pathname
      ,EX: E:\WINNT351 which is the path  where the setup file 
      OEMSETUP.INF is located, and then choose the OK button.

   6. The screen will appear "Duplex Mode" dialog box which is provide
      by DLKRTS.SYS driver. The default value is "auto" so that the
      D-Link DFE-538TX 10/100 Adapter and its driver DLKRTS.SYS will
      auto-detect the line speed, while the DLKRTS.SYS is loading. 

   7. NT will then perform the binding process. If any additional network
      software options were installed, you may be prompted for specific
      information for these packages.

   8. Restarting your system you will acquire network service.
   